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RPA crossing should be minimized.  One crossing is preferred.

Floodplain, RPA and wetlands should be clearly labeled and shown with consistent line codes on the plan of development.  If BMPs are anticipated to meet state and county standards, these locations should also be shown.  Show existing onsite pond.

No grading for BMPs will be allowed in the RPA.  Outfalls and RPA crossings must minimize RPA and wetland impacts.

For site plan

1) Wetlands delineation and if present, applicable permits from US Army Corps of Engineers required.
2) Identify RPA Areas.  No stormwater BMPs are allowed in RPA areas.
3) Water Quality Impact Assessment certifications required.  See WQIA forms available at https://www.hanovercounty.gov/DocumentCenter/View/163
4) Disturbance in floodplain will require a H&H study must meet encroachment provisions in Sect 26-235.15 of Hanover County Ordinance as follows.
“ Within any floodway area, no encroachments, including fill, new construction, substantial improvements, or other development shall be permitted unless it has been demonstrated through hydrologic and hydraulic analysis, performed in accordance with standard engineering practice, that the proposed encroachment will not result in any increase in flood levels within the county during the occurrence of the base flood. Hydrologic and hydraulic analyses shall be undertaken only by professional engineers or others of demonstrated qualifications, who shall certify that the technical methods used correctly reflect currently-accepted technical concepts. Studies, analyses, or computations shall be submitted in sufficient detail to allow a thorough review by the floodplain administrator.
Development activities which increase the water surface elevation of the base flood may be allowed, provided that the applicant first applies with the county's endorsement for a CLOMR, and receives FEMA approval.”
5) Plans must demonstrate that the site is less than 1% of drainage area at the outfall of the storm sewer system, or detention may be required.
6) Any ponds remaining onsite must meet Hanover county requirements.  Disposition of the pond and any associated wetland or other permitting to be addressed.

