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No comments on the CUP, comments are on future site plan:

1. Additional development subject to runoff reduction and channel protection.
2. With any increase in impervious area, it is likely that the onsite detention of stormwater will be required.
3. If development is 5 acres or more or 10lb or more of phos load, 75% of nutrient reduction must be met on site.
4. Analysis of downstream manmade and natural systems to a point where the site is less than 1% of drainage area will likely be required.
5. Currently approved construction plan allows for 0.57 acres of impervious.  Any additional impervious will need to be addressed with the development of the church property.  No increase in runoff to the pond would be allowed for the 2, 10, and 100 year storms.


